# Task 1

Plot a sine wave

# Code:

x = 0:pi/100:2\*pi;  
y = sin(x);  
plot(x,y)

# Output:

